| CrossManager V2026.2 |

Manual

# News

V2026.2

- Input
  - Catia V5 : Added support of version CATIA V5-6R2026
  - Fusion 360 : Added support of version 2606.1.36
  - PARASOLID : Added support of version 38.1
  - NX/Unigraphics : Added support for NX 2512 Series until version 2512.4000
  - ACIS : Improved management of file support for versions from 2021 1.0, improved management of file with several bodies and bad quality files
  - Creo Parametric : Additions in ModelDisplays (appearance, views in camera node), default colors now fixed with duplicated components
  - Inventor : Improved reading of metadata, improved management of files from Inventor 2024 and bad quality files
  - ZW3D : Added processing of metadata on nodes, various fixes
  - glTF : Added support of metadata
  - Revit : Improved facetted geometry handling
- Output
  - IFC : Added handling of open shells, translated as IFC face based surface model
  - glTF : Added configuration to write "embedded" glTF (binary inside glTF file), added writing of metadata in the nodes' "extra" field, additional "mesh" nodes only for the second mesh

V2026.1

- Input
  - ZW3D : NEW FORMAT, support of versions up to ZW3D 2026
  - CatiaV6/3DEXPERIENCE : Added support of version R2026x
  - SOLIDWORKS : Added support of version SOLIDWORKS 2026
  - Solid Edge : Added support for version Solid Edge 2026
  - Fusion 360 : Added support for version 2605.1.39
  - NX/Unigraphics : Added support for NX 2512 Series until version 2512.1700
  - QIF : Added UUID read for every component, node, and entity
  - JT : improved semantic PMIs
  - FBX : support of TGA texture
- Output
  - JT : faster conversion with versions 9.x and 10.x, optimized compression
  - 3dxml : Added management of Unicode file paths, folders and names

V2025.4

- Input
  - Creo Parametric : Added support of version Creo 12.0
  - Creo View : Added support of version Creo View 12.0
  - STEP : Added support for last published schema AP242.E4, support of persistent IDs (uuid) for topological and geometrical elements
  - PARASOLID : Added support of version 38.0
  - Fusion 360 : Added support of versions up to 2603.1.52
  - NX/Unigraphics : Added support for NX 2506 Series until 2506.4000
  - Navisworks : improved reading of properties
  - Catia V5 : improved reading of helicoidal surfaces, improved management of connectors for assembly PMI
- Output
  - STEP : Added support for last published schema AP242.E4
  - ACIS : Added writing of face name attributes

V2025.3

- Input
  - Inventor : Added support of version Inventor 2026
  - Fusion 360 : Added support of versions up to 2602.0.71
  - Navisworks : Added support of version Navisworks 2026
  - Revit : Added support of version Revit 2026, support of Revit assemblies
  - NX/Unigraphics : Added support for NX 2412 Series until 2412.7000
- Output
  - Catia V5 : Added support of version CATIA V5-6R2025
  - CGR : improved transparency writing

# Prelude

This documentation defines the whole features of the application CrossManager, designed to convert 2D and 3D models from a list of available input formats into one of the possible output formats.
(see table in appendix for available combinations : Appendix)

- To begin with
- CrossManager Overview
- Configure
- Appendix
- Licenses pages