| CrossManager V2026.2 |

Tessellation settings : [STL CONF]

Tessellation settings
[STL CONF]

## Configuration for Stl

Parameter | Default value | Usage | Format
--- | --- | --- | ---
MAXSIZE | 100000000000000010000000000000000000000000000000000.0000000 | maximun size of a triangle | double
MINSIZE | 0.0000000 | minimun size of a triangle | double
RATIO | 10000.0000000 | ratio between two side of a triangle ( maximun value ) | double
LINEAR_DIS | 1 | Disable linear tolerance ( 0=linear tolerance enable 1=linear tolerance disable) | boolean
LINEAR_TOL | 0.1000000 | linear tolerance value | double
ANGULAR_DIS | 1 | Disable angular tolerance ( 0=angular tolerance enable 1=angular tolerance disable) | boolean
ANGULAR_TOL | 0.174532 | angle value in radian | double
WRITE_ASCII | 0 | if 0 write a binary stl file if 1 write an ascii stl file | boolean
COMPUTE_NORMALS_FROM_SURFACE | 1 | if 1 compute the normal from surface 0 normal is an approximation of triangle (suggest 0 for STL writer , 1 for other writer) | boolean
USE_TESSEL | 1 | Should we use tesselation on body or mesh read in model [1] -> use tessel [0] -> use mesh read | boolean
COMPUTE_BOUNDARIES_FROM_MESH | 1 | Should we compute boundaries from mesh [1] -> Yes [0] -> No | boolean