| CrossManager V2026.2 |

[TRANSFORMING]
[TRANSFORMING]

## Configuration for Transforming

Parameter | Default value | Usage | Format
--- | --- | --- | ---
BODY_TO_NURBS | 0 | Should we convert all geometries to nurbs ? [1] -> Yes [0] -> No | boolean
KEEP_ASSEMBLY | 1 | Should we write the parts/assemblies (308/408 IGES) ? [1] -> Yes [0] -> No (flatten entities) | boolean
EXPLODE_GROUP | 1 | Should we write a group for faces in same solid? [1] -> No [0] -> Yes | boolean
MERGE_BODIES | 0 | Should we merge all bodies with only one face in one body ? (usefull for facetted and xmt writers) [1] -> Yes [0] -> No | boolean
MERGE_BODIES_BY_LAYER | 0 | Should we organise bodies by layers ? [1] -> Yes [0] -> No | boolean
REMOVE_EMPTY_NODES | 0 | Should we simplfy node tree? (Usefull for pdf writer) [0](Default) -> keep complete tree [1] -> remove leaf node which does not contain any 3D data | boolean