| CrossManager V2025.4 |

[JT CONF]
[JT CONF]

## Configuration for Jt

Parameter | Default value | Usage | Format
--- | --- | --- | ---
WRITE_XTBREP | 0 | Should we write ParasolidBRep in the JT file ? [1] -> Yes [0] -> No (default) | boolean
WRITE_RELEASE | 95 | Version output [80] -> version 8.0 (default) [90] -> version 9.0, (...) [95] -> version 9.5 [100] -> version 10.0, (...) [107] -> version 10.7 | integer
WRITE_EXPORT_TYPE | 0 | Export type [0] -> Monolithic (default) [1] -> Shattered [2] -> PerPart | boolean
WRITE_STRATEGY | 1 | Assembly strategy [0] -> Write components only (default) [1] -> Write components and filled nodes | boolean
JT_PMI_AS_SEMANTIC | 0 | Should we read PMI as semantic [1] -> Yes [0] -> No (default, graphical) | boolean
READ_BOUND_PREFERENCE | 3 | Which boundary curves should we prefere for JT-Brep topology ? [2] : Priority to UV boundary curves [3] : Priority to 3D boundary curves | integer