| CrossManager V2025.4 |

[STEP CONF]
[STEP CONF]

## Configuration for Step

Parameter | Default value | Usage | Format
--- | --- | --- | ---
FDT_REPRESENTATION | 1 | What representation mode for FDT ? [0] -> Only "frozen" graphical information (3D tessellation or polylines) [1] -> Full semantics, with given priority to "frozen" graphical information [2] -> Full semantics, with given priority to the "placeholder" graphical information (receiving system is in charge of recreating graphics based on it) | integer
READ_COMPONENT_NAME | 1 | Gives priority to specific STEP PRODUCT fields for Dtk_Component naming [0] -> Considers only PRODUCT.ID [1] -> Gives priority to PRODUCT.ID, over PRODUCT.NAME, if not empty [2] -> Gives priority to PRODUCT.NAME, over PRODUCT.ID, if not empty [3] -> Concatenates PRODUCT.ID and PRODUCT.NAME (if different) | integer
READ_EXTENDED_ASCII | 0 | Choose code page or encoding to be used in case of non-standard ASCII characters encountered [0] -> UTF-8 [1] -> Code page 936 (Microsfot Windows, simplified chinese) [2] -> Code page 855 (Cyrillic) | integer
READ_COLOR_UNLISTED | 2 | Should we read non-correctly defined colors (not in a list) ? [0] -> No [1] -> If some colors are correctly defined, ignore only those non-correctly defined [2] -> Yes | integer
READ_ORPHAN_BODY | 3 | Should we read orphan bodies (not attached to a product) ? [0] -> No [1] -> Only if no product is defined [2] -> Only if no product is defined, or several products are defined but no assembly [3] -> Yes | integer
WRITE_VERSION | 4 | Writes Step Version [0] -> AP214 if WRITE_FDT=0, AP242E1 otherwise [1] -> AP203 [2] -> AP214 [3] -> AP203E2 [4] -> AP242E1 [5] -> AP242E4 | integer
WRITE_FDT | 1 | Drives Writing of FDT [0] -> No [1] -> semantic + graphic [-1] -> graphic only | integer
WRITE_FDT_POLYLINE | 0 | Selects mode for graphic output [-1] deprecated -> character based [0] -> default (same as [2]) [1] -> minimal graphic (known as "placeholder") [2] -> 3D polyline [3] -> 2D tesselation [4] -> 3D tesselation | integer
WRITE_ITEMNAME | 3 | Writes Names of Items (topological items) [0] -> No (empty name) [1] -> name from CAD if defined, else empty [2] -> "nÂ° iii" : ID from CAD [3] -> "no iii" : ID from CAD | integer
WRITE_PROPERTY | 2 | Writes Attributes and Properties [0] -> no [1] -> Product Data [2] -> also general attributes (metadata) except "File Property" [3] -> all general attributes, also "File Property" | integer
VALIDATION_PROPERTY | 0 | Drives Computing/Checking of Validation Propeties (Read & Write) [0] -> No [1] -> computes simple validation properties [2] -> computes geometric validation properties (except clouds of points) [3] -> computes also clouds of points | integer
WRITE_LENGTH_UNIT | 0 | Controls Length Unit on Writing [0] -> keeps original unit : MM (default) [between 1 and 6] -> changes writing unit and converts data from MM [1] -> MM [2] -> CM [3] -> M [4] -> KM [5] -> INCH [6] -> FOOT | integer
WRITE_COMPRESS | 0 | Controls Writing of Compressed Step Files [0] -> No [1] -> Yes | integer
WRITE_MESH | 0 | Controls writing of geometry as is or converted to Mesh [0] -> write geometry as is [1] -> convert geometry to mesh when writing | integer
WRITE_EXTREF | 0 | Controls writing of an assembly with external references [0] -> No (monolithic file) [1] -> Per Part (one file per leaf component + one file for the whole assembly set) [2] -> Nested (one file per component, whether leaf, sub-assembly, main assembly) | integer