| CrossManager V2026.2 |

[IFCW CONF]
[IFCW CONF]

## Configuration for Ifcw

Parameter | Default value | Usage | Format
--- | --- | --- | ---
IFC_VERSION | 1 | IFC version to write ? [0] -> IFC2X3 [1] -> IFC4 | integer
BUILDINGTYPE_RECOGNITION | 1 | Enable recognition of IFC building element subtype ? [0] -> No, element with geometry will be written as IFCBUILDINGELEMENTPROXY [1] -> Yes | boolean