| CrossManager V2026.3 |

Manual

# News

V2026.3

- Input
  - ACIS :
    - Added support for versions up to 2025 1.0
    - Improved management of invalid files
  - Creo Parametric : Added support for version Creo Parametric 13.0
  - FBX : Added support for ObjectMetadatas
  - Fusion 360 : Added support for versions up to 2703.1.11
  - Inventor : Added support for version Inventor 2027
  - JT : Improved reading of semantic PMI for feature control frames, datum, notes
  - Navisworks : Added support for version Navisworks 2027
  - NX/Unigraphics : Added support for NX 2606 Series until version 2606.1700
  - Revit : Added support for version Revit 2027
  - SOLIDWORKS : Added support for version SOLIDWORKS 2026 SP2.1
  - USD :
    - NEW FORMAT, support for versions from 0.8.0 to 0.9.0
    - Supports .usd binary and ASCII files
  - ZW3D : Added support for version ZW3D 2026 SP2
- Output
  - Catia V5 : Added support for version CATIA V5-6R2026
  - FBX : Added support for ObjectMetadatas
  - IFC : Added georeferencing handling support (site latitude, longitude and elevation e.g. Revit Project Base Point), added instance color override handling
  - JT :
    - Added support for texture images with transparent background
    - Added semantic data for PMI for Feature Control Frame, Datum, Balloon, Note
  - STEP : Added handling for customer defined attributes at part, product and geometry/topology level

V2026.2

- Input
  - Catia V5 : Added support of version CATIA V5-6R2026
  - Fusion 360 : Added support of version 2606.1.36
  - PARASOLID : Added support of version 38.1
  - NX/Unigraphics : Added support for NX 2512 Series until version 2512.4000
  - ACIS : Improved management of file support for versions from 2021 1.0, improved management of file with several bodies and bad quality files
  - Creo Parametric : Additions in ModelDisplays (appearance, views in camera node), default colors now fixed with duplicated components
  - Inventor : Improved reading of metadata, improved management of files from Inventor 2024 and bad quality files
  - ZW3D : Added processing of metadata on nodes, various fixes
  - glTF : Added support of metadata
  - Revit : Improved facetted geometry handling
- Output
  - IFC : Added handling of open shells, translated as IFC face based surface model
  - glTF : Added configuration to write "embedded" glTF (binary inside glTF file), added writing of metadata in the nodes' "extra" field, additional "mesh" nodes only for the second mesh

V2026.1

- Input
  - ZW3D : NEW FORMAT, support of versions up to ZW3D 2026
  - CatiaV6/3DEXPERIENCE : Added support of version R2026x
  - SOLIDWORKS : Added support of version SOLIDWORKS 2026
  - Solid Edge : Added support for version Solid Edge 2026
  - Fusion 360 : Added support for version 2605.1.39
  - NX/Unigraphics : Added support for NX 2512 Series until version 2512.1700
  - QIF : Added UUID read for every component, node, and entity
  - JT : Improved semantic PMIs
  - FBX : Added support of TGA texture
- Output
  - JT : Improved faster conversion with versions 9.x and 10.x, optimized compression
  - 3dxml : Added management of Unicode file paths, folders and names

V2025.4

- Input
  - Creo Parametric : Added support of version Creo 12.0
  - Creo View : Added support of version Creo View 12.0
  - STEP : Added support for last published schema AP242.E4, support of persistent IDs (uuid) for topological and geometrical elements
  - PARASOLID : Added support of version 38.0
  - Fusion 360 : Added support of versions up to 2603.1.52
  - NX/Unigraphics : Added support for NX 2506 Series until 2506.4000
  - Navisworks : Improved reading of properties
  - Catia V5 : Improved reading of helicoidal surfaces, improved management of connectors for assembly PMI
- Output
  - STEP : Added support for last published schema AP242.E4
  - ACIS : Added writing of face name attributes

# Prelude

This documentation defines the whole features of the application CrossManager, designed to convert 2D and 3D models from a list of available input formats into one of the possible output formats.
(see table in appendix for available combinations : Appendix)

- To begin with
- CrossManager Overview
- Configure
- Appendix
- Licenses pages