| CrossManager V2026.2 |

[IGES CONF]
[IGES CONF]

## Configuration for Iges

Parameter | Default value | Usage | Format
--- | --- | --- | ---
NAME_AS_406 | 0 | Should we write the name of an entity as a 406 ? [1] -> Yes [0] -> No We should use 1 (except if we are using the old writing style) | boolean
BOUND_PREFERENCE | 2 | Which boundary curves should we read ? [2] : Priority to UV boundary curves [3] : Priority to 3D boundary curves | integer
READ_AS_DRAWING | 0 | Should we read all file as a drawing ? [1] -> Yes [0] -> No | integer
READ_STRING_DECODING | 0 | Choose code page or encoding to be used in case of non-standard ASCII characters encountered [0] -> Use text as it is [1] -> Convert from UTF-8 [2] -> Convert using JIIS [3] -> Convert using Code page 936 (Microsfot Windows, simplified chinese) | integer