| CrossManager V2025.4 |

[DOMAIN FILTERING]
[DOMAIN FILTERING]

## Configuration for Domain filtering

Parameter | Default value | Usage | Format
--- | --- | --- | ---
TRIM_CURVES | 0 | Which trimming curves should we setup ? [0] : Default ( As they are) [1] : Only 2D curves [2] : Boths 2D+3D [3] : Only 3D curves | integer
SOLID | 0 | Should we ignore Solid entities ? (only for independant entities) [1] -> Yes [0] -> No | boolean
WIREFRAME | 0 | Should we ignore wire entities ? (only for independant entities) [1] -> Yes [0] -> No | boolean
FDT | 0 | Should we ignore FDT/PMI entities ? (only for independant entities) [1] -> Yes [0] -> No | boolean
FEATURES | 1 | Should we ignore feature entities ? (only for independant entities) [1] -> Yes [0] -> No | boolean
META_PARAMETERS | 0 | Should we ignore meta data ? [1] -> Yes [0] -> No | boolean
REFERENCE_AXIS | 1 | Should we ignore reference axis ? [1] -> Yes [0] -> No | boolean
MESH | 1 | Should we ignore meshes ? [1] -> Yes [0] -> No | boolean
RENDER_INFOS | 1 | Should we ignore render infos ? [1] -> Yes (use basis color) [0] -> No | boolean
DRAW | 0 | Should we ignore drawing (2D entities) ? [1] -> Yes [0] -> No | boolean
CONSTRUCT_SOLIDS | 1 | Should we ignore construction geometry ? [1] -> Yes [0] -> No | boolean
INFINITE_GEOMETRY | 1 | Should we ignore infinite geometry ? [1] -> Yes [0] -> No | boolean
GEOM_LINK | 1 | Should we ignore geometrical links for highlightning? [1] -> Yes [0] -> No | boolean
MODEL_DISPLAY | 1 | Should we ignore model displays? [1] -> Yes [0] -> No | boolean
CAMERA | 0 | Should we ignore model camera? [0] -> No [1] -> Yes [2] -> Ignores only inactive cameras | integer
ANNOTATION_VIEW | 0 | Should we ignore annotation view? [1] -> Yes [0] -> No | boolean