| CrossManager V2025.4 |

[XMT CONF] - Parasolid
[XMT CONF]

## Configuration for Xmt

Parameter | Default value | Usage | Format
--- | --- | --- | ---
WRITE_BODY_ATTRIBUTES | 1 | Should we write body attributes ? [0] -> No [1] -> Yes [-1] -> Yes and all bodies attributs are updated by the part attibuts [-2] -> Yes and all bodies name are updated by part name [-3] -> Yes and all bodies without name are updated by part name [-4] -> Yes and all bodies without name are updated by previous node name or part name | integer
USE_PART_NAME | 0 | Should we set the part attribut to the unique body ? [0] -> No [1] -> Yes all the part attributs update body attributs [2] -> Yes but only the part name update body name [3] -> Yes but only body without name are updated by the part name [4] -> Yes but only body without name are updated by previous node name or part name | integer